Evaluation OCR

Data Asli:

1. Slide One

Esco Ductless Fume Hoods

KEY FEATURES:

The “GREEN” solution

Safe Carbon Filtration

Low installation and maintenance cost

Ergonomic

ISOCIDE™ antimicrobial powder coating

2. Slide 2

OVERVIEW OF MODELS

Ascent™ Max Series

Standard model Model: ADC-B

Main Filter: Carbon

Has an option for motorized sash

Available sizes: 2, 3, 4, 5, 6 ft. With Secondary Carbon Filter Model: ADC-C

Main Filter : Carbon Secondary Filter: Carbon

Available sizes: 3, 4, 5, 6 ft. With Secondary HEPA Filter Model: ADC-E

Main Filter : Carbon Secondary Filter: HEPA

Available sizes: 3, 4, 5, 6 ft

ADC’s worktop may be upgraded to: - Epoxy - Phenolic Resi

OPTIONS AND ACCESSORIES

Carbon Filter (Type A-Type H) Electrical Outlet VOC Sensor American Style Service Fixture

Swan-neck faucet and PP Drip Cup European Style Service Fixture Base Cabinet Support Stand with Leveling Feet Support Stand with Caster Wheels

3. Slide 3

Ascent™ Opti Series

Model: SPD-A

Main Filter: Carbon Filter

Double hinged sash mechanism

Includes a mobile cart, no sink

Available sizes: 3 and 4 ft. Model: SPD-B

Main Filter: Carbon Filter

Double hinged sash mechanism

Transparent back wall made of acrylic

Includes a mobile cart, no sink

Available sizes: 3 and 4 ft

Ascent™ Opti Formax

Model: SPF

Double hinged sash

Formalin-dispensing Fumehood

Removes formalin fumes through carbon filtration

Available sizes: 3 and 4 ft.

Ascent™ Opti Titramax

Model: SPT

Horizontal sliding sash

Phenolic resin worktop

Main filter: Carbon filter

Available Sizes: 3 and 4 ft

Ascent™ Filtered Storage Cabinet

Model: ASC-\_ Fumes from chemical containers often result to the storage cabinet’s corrosion and contaminated air in the laboratory. Ascent™ storage cabinet is ideal in providing a safe and convenient storage solution. This cabinet is equipped with Nanocarb™ filters that effectively adsorb chemical fumes to provide operator and environment protection.

Has Polypropylene trays

Sentinel™ microprocessor controller

Door safety lock restricts access

Multiple filter configurations

Available sizes: 2, 4, 6 ft